# Menu 11 Single Line Descriptions − Miscellaneous

Mode: Open‑Loop

Parameter | Range | Default | Type
--- | --- | --- | ---
11.001 | Option Synchronisation Select | Not Active (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Automatic (5) | Slot 3 (3) | RW | Txt |  |  |  | US
11.002 | Option synchronisation Active | Not Active (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) |  | RO | Txt | ND | NC | PT |
11.017 | Keypad Defined Node Address | -2147483648 to 2147483647 | 0 | RO | Num |  | NC | PT | PS
11.018 | Status Mode Parameter 1 | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
11.019 | Status Mode Parameter 2 | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
11.020 | Reset Serial Communications | Off (0) or On (1) |  | RW | Bit | ND | NC |  |
11.021 | Parameter 00.030 Scaling | 0.000 to 10.000 | 1.000 | RW | Num |  |  |  | US
11.022 | Parameter Displayed At Power‑up | 0.000 to 0.080 | 0.010 | RW | Num |  |  | PT | US
11.023 | Serial Address | 1 to 247 | 1 | RW | Num |  |  |  | US
11.024 | Serial Mode | 8 2 NP (0), 8 1 NP (1), 8 1 EP (2), 8 1 OP (3), 8 2 NP M (4), 8 1 NP M (5), 8 1 EP M (6), 8 1 OP M (7), 7 2 NP (8), 7 1 NP (9), 7 1 EP (10), 7 1 OP (11), 7 2 NP M (12), 7 1 NP M (13), 7 1 EP M (14), 7 1 OP M (15) | 8 2 NP (0) | RW | Txt |  |  |  | US
11.025 | Serial Baud Rate | 300 (0), 600 (1), 1200 (2), 2400 (3), 4800 (4), 9600 (5), 19200 (6), 38400 (7), 57600 (8), 76800 (9), 115200 (10) | 19200 (6) | RW | Txt |  |  |  | US
11.026 | Minimum Comms Transmit Delay | 0 to 250 ms | 2 ms | RW | Num |  |  |  | US
11.027 | Silent Period | 0 to 250 ms | 0 ms | RW | Num |  |  |  | US
11.028 | Drive Derivative | 0 to 255 |  | RO | Num | ND | NC | PT |
11.029 | Software Version | 0 to 99999999 |  | RO | Num | ND | NC | PT |
11.030 | User Security Code | 0 to 2147483647 |  | RW | Num | ND | NC | PT | US
11.031 | User Drive Mode | Open‑loop (1), RFC‑A (2), RFC‑S (3), Regen (4) |  | RW | Txt | ND | NC | PT |
11.032 | Maximum Heavy Duty Rating | 0.000 to 99999.999 A |  | RO | Num | ND | NC | PT |
11.033 | Drive Rated Voltage | 200V (0), 400V (1), 575V (2), 690V (3) |  | RO | Txt | ND | NC | PT |
11.034 | Software Sub‑version | 0 to 99 |  | RO | Num | ND | NC | PT |
11.036 | NV Media Card File Previously Loaded | 0 to 999 | 0 | RO | Num |  | NC | PT |
11.037 | NV Media Card File Number | 0 to 999 | 0 | RW | Num |  |  |  |
11.038 | NV Media Card File Type | None (0), Open‑loop (1), RFC‑A (2), RFC‑S (3), Regen (4), User Prog (5) |  | RO | Txt | ND | NC | PT |
11.039 | NV Media Card File Version | 0 to 9999 |  | RO | Num | ND | NC | PT |
11.040 | Customer Specific Parameter | 0 to 0 | 0 | RO | Num |  | NC | PT |
11.041 | NV Media Card Disable Booting | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
11.042 | Parameter Cloning | None (0), Read (1), Program (2), Auto (3), Boot (4) | None (0) | RW | Txt |  | NC |  | US
11.043 | Load Defaults | None (0), Standard (1), US (2) | None (0) | RW | Txt |  | NC |  |
11.044 | User Security Status | Menu 0 (0), All Menus (1), Read‑only Menu 0 (2), Read‑only (3), Status Only (4), No Access (5) |  | RW | Txt | ND |  | PT |
11.045 | Select Motor 2 Parameters | Motor 1 (0), Motor 2 (1) | Motor 1 (0) | RW | Txt |  |  |  | US
11.046 | Defaults Previously Loaded | 0 to 2000 |  | RO | Num | ND | NC | PT | US
11.047 | Onboard User Program: Enable | Reset And Run (-1), Stop (0), Run (1) | Run (1) | RW | Txt |  |  |  | US
11.048 | Onboard User Program: Status | Stopped (0), Running (1), Exception (2), No Program (3) |  | RO | Txt | ND | NC | PT |
11.049 | Onboard User Program: Programming Events | 0 to 65535 |  | RO | Num | ND | NC | PT |
11.050 | Onboard User Program: Freewheeling Tasks Per Second | 0 to 65535 |  | RO | Num | ND | NC | PT |
11.051 | Onboard User Program: Clock Task Time Used | 0.0 to 100.0 % |  | RO | Num | ND | NC | PT |
11.052 | Serial Number LS | 000000000 to 999999999 |  | RO | Num | ND | NC | PT |
11.053 | Serial Number MS | 0 to 999999999 |  | RO | Num | ND | NC | PT |
11.054 | Drive Date Code | 0 to 65535 |  | RO | Num | ND | NC | PT |
11.055 | Onboard User Program: Clock Task Scheduled Interval | 0 to 262140 ms |  | RO | Num | ND | NC | PT |
11.059 | Minimum No‑overload Current | 0.000 to 99999.999 A |  | RO | Num | ND | NC | PT |
11.060 | Maximum Rated Current | 0.000 to 99999.999 A |  | RO | Num | ND | NC | PT |
11.061 | Full Scale Current Kc | 0.000 to 99999.999 A |  | RO | Num | ND | NC | PT |
11.062 | Power Board Software Version Number | 0.00 to 99.99 |  | RO | Num | ND | NC | PT |
11.063 | Product Type | 0 to 255 |  | RO | Num | ND | NC | PT |
11.064 | Product Identifier Characters | 1295463729 to 2147483647 |  | RO | Num | ND | NC | PT |
11.065 | Drive Rating And Configuration | 00000000 to 99999999 |  | RO | Num | ND | NC | PT |
11.066 | Power Stage Identifier | 0 to 255 |  | RO | Num | ND | NC | PT |
11.067 | Control Board Identifier | 0.000 to 65.535 |  | RO | Num | ND | NC | PT |
11.068 | Internal I/O Identifier | 0 to 255 |  | RO | Num | ND | NC | PT |
11.069 | Position Feedback Interface Identifier | 0 to 255 |  | RO | Num | ND | NC | PT |
11.070 | Core Parameter Database Version | 0.00 to 99.99 |  | RO | Num | ND | NC | PT |
11.072 | NV Media Card Create Special File | 0 to 1 | 0 | RW | Num |  | NC |  |
11.073 | NV Media Card Type | None (0), SMART Card (1), SD Card (2) |  | RO | Txt | ND | NC | PT |
11.075 | NV Media Card Read‑only Flag | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
11.076 | NV Media Card Warning Suppression Flag | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
11.077 | NV Media Card File Required Version | 0 to 9999 |  | RW | Num | ND | NC | PT |
11.078 | NV Media Card Action Status | None (0), Active (1), Card Slot 1 (2), Card Slot 2 (3), Card Slot 3 (4), Card Slot 4 (5), Card Product (6), Card User Prog (7), Card Busy (8), Card Data Exists (9), Card Option (10), Card Read Only (11), Card Error (12), Card No Data (13), Card Full (14), Card File Error (15), Card Rating (16), Card File Data (17), Card Derivative (18) |  | RO | Txt | ND | NC | PT |
11.079 | Drive Name Characters 1‑4 | -2147483648 to 2147483647 | 0 | RW | Num |  |  | PT | US
11.080 | Drive Name Characters 5‑8 | -2147483648 to 2147483647 | 0 | RW | Num |  |  | PT | US
11.081 | Drive Name Characters 9‑12 | -2147483648 to 2147483647 | 0 | RW | Num |  |  | PT | US
11.082 | Drive Name Characters 13‑16 | -2147483648 to 2147483647 | 0 | RW | Num |  |  | PT | US
11.084 | Drive Mode | Open‑loop (1), RFC‑A (2), RFC‑S (3), Regen (4) |  | RO | Txt | ND | NC | PT | US
11.085 | Security Status | None (0), Read‑only (1), Status‑only (2), No Access (3) |  | RO | Txt | ND | NC | PT | PS
11.086 | Menu Access Status | Menu 0 (0), All Menus (1) |  | RO | Txt | ND | NC | PT | PS
11.090 | Keypad Port Serial Address | 1 to 16 | 1 | RW | Num |  |  |  | US
11.091 | Additional Identifier Characters 1 | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.092 | Additional Identifier Characters 2 | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.093 | Additional Identifier Characters 3 | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |