# Slot 3 Menu 9 Single Line Descriptions − Resources

Mode: Open‑Loop

Parameter | Range | Default | Type
--- | --- | --- | ---
3.09.009 | Background period | 0 to 65535 ms |  | RO | Num | ND | NC | PT |
3.09.010 | PreCritical Task % Free | -128 to 100 % |  | RO | Num | ND | NC | PT |
3.09.011 | Critical Task % Free | -128 to 100 % |  | RO | Num | ND | NC | PT |
3.09.012 | PostCritical Task % Free | -128 to 100 % |  | RO | Num | ND | NC | PT |
3.09.020 | PreCritical Task Worst % Free | -128 to 100 % |  | RO | Num | ND | NC | PT |
3.09.021 | Critical Task Worst % Free | -128 to 100 % |  | RO | Num | ND | NC | PT |
3.09.022 | PostCritical Task Worst % Free | -128 to 100 % |  | RO | Num | ND | NC | PT |
3.09.024 | OutData Margin | -2147483648 to 2147483647 µs |  | RO | Num | ND | NC | PT |
3.09.030 | PCB Temperature | -128 to 127 °C |  | RO | Num | ND | NC |  |
3.09.039 | Active Alarm Bits | 0000000000000000 to 1111111111111111 |  | RO | Bin | ND | NC | PT |
3.09.040 | Diagnostic Counter Selector | Off (0), Port A Inv Errs (1), Port B Inv Errs (2), Port A Rx Errs (3), Port B Rx Errs (4), Port A Fwd Errs (5), Port B Fwd Errs (6), Port A LL Count (7), Port B LL Count (8), SPI CRC Errs (9), SPI Start Errs (10), SPI NACK Errs (11), SPI Retry Count (12), SPI Req Count (13), Internal 1 (14), Internal 2 (15), Internal 3 (16) | Off (0) | RW | Txt |  | NC | PT |
3.09.041 | Diagnostic Counter Value | 0 to 0 |  | RO | Num | ND | NC | PT |
3.09.043 | Worst Drive to Network Sync time | 0 to 65535 ms |  | RW | Num | ND | NC | PT |
3.09.050 | Object Index view Selector 1 | 0 to 65535 | 0 | RW | Num |  | NC | PT |
3.09.051 | Object Subindex View Selector 1 | 0 to 255 | 0 | RW | Num |  | NC | PT |
3.09.052 | Object view value 1 | 0 to 0 |  | RO | Num | ND | NC | PT |
3.09.053 | Object Index view Selector 2 | 0 to 65535 | 0 | RW | Num |  | NC | PT |
3.09.054 | Object Subindex View Selector 2 | 0 to 255 | 0 | RW | Num |  | NC | PT |
3.09.055 | Object view value 2 | 0 to 0 |  | RO | Num | ND | NC | PT |
3.09.056 | Object Index view Selector 3 | 0 to 65535 | 0 | RW | Num |  | NC | PT |
3.09.057 | Object Subindex View Selector 3 | 0 to 255 | 0 | RW | Num |  | NC | PT |
3.09.058 | Object view value 3 | 0 to 0 |  | RO | Num | ND | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |