# Menu 7 Single Line Descriptions − Analog I/O

Mode: RFC‑A

Parameter | Range | Default | Type
--- | --- | --- | ---
07.001 | Analog Input 1 | ±100.00 % |  | RO | Num | ND | NC | PT | FI
07.004 | Monitored Temperature 1 | ±250 °C |  | RO | Num | ND | NC | PT |
07.005 | Monitored Temperature 2 | ±250 °C |  | RO | Num | ND | NC | PT |
07.006 | Monitored Temperature 3 | ±250 °C |  | RO | Num | ND | NC | PT |
07.008 | Analog Input 1 Scaling | 0.000 to 10.000 | 1.000 | RW | Num |  |  |  | US
07.009 | Analog Input 1 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
07.010 | Analog Input 1 Destination | 0.000 to 59.999 | 1.036 | RW | Num | DE |  | PT | US
07.025 | Calibrate Analog Input 1 Full Scale | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
07.026 | Analog Input 1 Fast Update Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
07.030 | Analog Input 1 Offset | ±100.00 % | 0.00 % | RW | Num |  |  |  | US
07.033 | Power Output | ±100.0 % |  | RO | Num | ND | NC | PT |
07.034 | Inverter Temperature | ±250 °C |  | RO | Num | ND | NC | PT |
07.035 | Percentage Of d.c. Link Thermal Trip Level | 0 to 100 % |  | RO | Num | ND | NC | PT |
07.036 | Percentage Of Drive Thermal Trip Level | 0 to 100 % |  | RO | Num | ND | NC | PT |
07.037 | Temperature Nearest To Trip Level | 00000 to 20999 |  | RO | Num | ND | NC | PT |
07.038 | Temperature Monitor Select 1 | 00000 to 10000 | 01001 | RW | Num |  |  |  | US
07.039 | Temperature Monitor Select 2 | 00000 to 10000 | 01002 | RW | Num |  |  |  | US
07.040 | Analog Input 1 Minimum | ±100.00 % | -100.00 % | RW | Num |  |  |  | US
07.043 | Analog Input 1 Maximum | ±100.00 % | 100.00 % | RW | Num |  |  |  | US
07.051 | Analog Input 1 Full Scale | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
07.052 | Temperature Monitor Select 3 | 00000 to 10000 | 00001 | RW | Num |  |  |  | US
07.063 | Analog Input 1 Filter Time Constant | Disabled (0), 500us (1), 1ms (2), 2ms (3), 4ms (4), 8ms (5), 16ms (6) | Disabled (0) | RW | Txt |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |