# Menu 3 Single Line Descriptions − Regen Set-up

Mode: Regeneration

Parameter | Range | Default | Type
--- | --- | --- | ---
03.001 | Reactive Power | VM_POWER[MIN] to VM_POWER[MAX] kVAr |  | RO | Num | ND | NC | PT | FI
03.003 | Charge System Present | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US
03.004 | Regen Synchronisation Mode | Re‑synchronise (0), Delayed Trip (1), Immediate Trip (2), Auto‑synchronise (3) | Re‑synchronise (0) | RW | Txt |  |  |  | US
03.005 | D.c. Voltage Set Point | VM_DC_VOLTAGE_SET[MIN] to VM_DC_VOLTAGE_SET[MAX] V | 200V drive: 350 V 400V drive: 700 V | RW | Num |  | RA |  | US
03.006 | D.c. Voltage Controller Proportional Gain Kp | 0 to 65535 | 4000 | RW | Num |  |  |  | US
03.007 | Disable Charge System / Close Contactor | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
03.008 | Charge System Disabled / Contactor Closed | Off (0) or On (1) |  | RO | Bit | ND | NC |  |
03.009 | Synchronised | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
03.010 | Power Input 1 | ±100.0 % | 0.0 % | RW | Num |  | NC |  |
03.011 | Current Trim Mode | Power‑up (0), On Enable (1), Disconnect Mode (2) | Power‑up (0) | RW | Txt |  |  |  | US
03.012 | Power Input Mode | Feed‑forward (0), kW Feed‑forward (1), Power kW (2) | Feed‑forward (0) | RW | Txt |  |  |  | US
03.013 | Power Input 2 | ±100.0 % | 0.0 % | RW | Num |  | NC |  |
03.014 | Power Input 3 | ±100.0 % | 0.0 % | RW | Num |  | NC |  |
03.015 | Power Input 1 Scaling | 0.000 to 4.000 | 1.000 | RW | Num |  |  |  | US
03.016 | Power Input 2 Scaling | 0.000 to 4.000 | 1.000 | RW | Num |  |  |  | US
03.017 | Power Input 3 Scaling | 0.000 to 4.000 | 1.000 | RW | Num |  |  |  | US
03.018 | Power Input kW | VM_POWER[MIN] to VM_POWER[MAX] kW | 0.000 kW | RW | Num |  | NC |  |
03.019 | Reactive Power Input Mode | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
03.020 | Reactive Power Input kVAR | VM_POWER[MIN] to VM_POWER[MAX] kVAr | 0.000 kVAr | RW | Num |  | NC |  | US
03.021 | Harmonic Reduction Enable | Disabled (0), Imbalance Only (1), All (2) | Imbalance Only (1) | RW | Txt |  |  |  | US
03.022 | D.c. Voltage Ramp Time | 0.1 to 100.0 V/ms | 1.0 V/ms | RW | Num |  |  |  | US
03.023 | Supply Loss Threshold | VM_AC_VOLTAGE_SET[MIN] to VM_AC_VOLTAGE_SET[MAX] V | 200V drive: 75 V 400V drive: 150 V | RW | Num |  | RA |  | US
03.024 | Minimum Supply Frequency | 10 to 195 Hz | 40 Hz | RW | Num |  |  |  | US
03.025 | Maximum Supply Frequency | 15 to 200 Hz | 70 Hz | RW | Num |  |  |  | US
03.026 | Minimum Supply Voltage | VM_AC_VOLTAGE[MIN] to VM_AC_VOLTAGE[MAX] V | 0 V | RW | Num |  | RA |  | US
03.027 | Maximum Supply Voltage | VM_AC_VOLTAGE[MIN] to VM_AC_VOLTAGE[MAX] V | 0 V | RW | Num |  | RA |  | US
03.028 | Supply Voltage | VM_AC_VOLTAGE_SET[MIN] to VM_AC_VOLTAGE_SET[MAX] V | 200V drive: 230 V 400V drive 50Hz: 400 V 400V drive 60Hz: 460 V | RW | Num |  | RA |  | US
03.029 | Supply Voltage Detection Mode | Measured dc (0), User (1), Measured dc (2), Measured ac (3) | Measured dc (0) | RW | Txt |  |  |  | US
03.030 | Island Detection Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
03.031 | Island Detection Injection Frequency | 1Hz (0), 2Hz (1), 4Hz (2) | 1Hz (0) | RW | Txt |  |  |  | US
03.032 | Island Detection Level | 0 to 1000 % |  | RO | Num | ND | NC | PT |
03.033 | Island Detection Synchronisation Source Select | Converter (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) | Converter (0) | RW | Txt |  |  |  | US
03.034 | Island Detect Synchronisation Source | Converter (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) |  | RO | Txt | ND | NC | PT |
03.035 | Synchronisation Headroom | 0.0 to 25.0 % | 5.0 % | RW | Num |  |  |  | US
03.036 | Estimated Supply Voltage | VM_AC_VOLTAGE[MIN] to VM_AC_VOLTAGE[MAX] V |  | RO | Num | ND | NC | PT | FI
03.037 | Positive Phase Sequence Volts | VM_AC_VOLTAGE[MIN] to VM_AC_VOLTAGE[MAX] V |  | RO | Num | ND | NC | PT | FI
03.038 | Negative Phase Sequence Volts | VM_AC_VOLTAGE[MIN] to VM_AC_VOLTAGE[MAX] V |  | RO | Num | ND | NC | PT | FI
03.039 | Negative Phase Sequence Current Gain | 0.00 to 1.00 | 0.05 | RW | Num |  |  |  | US
03.040 | Phase Imbalance Threshold | 0.0 to 50.0 % | 5.0 % | RW | Num |  |  |  | US
03.041 | Supply Loss Voltage | VM_AC_VOLTAGE[MIN] to VM_AC_VOLTAGE[MAX] V |  | RO | Num | ND | NC | PT | FI

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |