# Slot 3 Menu 1 Single Line Descriptions − User Application

Mode: Regeneration

Parameter | Range | Default | Type
--- | --- | --- | ---
3.01.003 | Program Status | None (0), Stopped (1), Run (2), Error (3) |  | RO | Txt | ND | NC | PT |
3.01.004 | Available CPU Resources | 0 to 100 % |  | RO | Num | ND | NC | PT |
3.01.013 | Auto‑run enable | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US
3.01.014 | Global runtime trip enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
3.01.015 | Disable reset on trip clear | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
3.01.017 | Enable out of range error | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
3.01.019 | Save user save params | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
3.01.020 | Power down retain data save | Save at UV (0), No Save (1), Force Save (2) | Save at UV (0) | RW | Txt |  |  |  | US
3.01.030 | Event 0 task schedule reason | 0 to 65535 |  | RO | Num | ND | NC | PT |
3.01.031 | Event 1 task schedule reason | 0 to 65535 |  | RO | Num | ND | NC | PT |
3.01.032 | Event 2 task schedule reason | 0 to 65535 |  | RO | Num | ND | NC | PT |
3.01.033 | Event 3 task schedule reason | 0 to 65535 | 0 | RO | Num |  | NC | PT |
3.01.049 | Run Time Error Code | No error (0), Param not exist (1), Param read‑only (2), Param write‑only (3), Param over range (4), Param dec places (5), Param type (6), Param no 64‑bit (7), Array bounds (8), Pointer alignmt (9), Pointer address (10), DINT div err (11), LINT div err (12), LREAL div err (13), REAL div err (14), DINT range err (15), UDINT range err (16), User Requested (17), Watchdog err (18), FPU instruct err (19), PosTask config (20), Reserved (21), Reserved (22), Reserved (23), Reserved (24), APC error (25), Reserved (26), Reserved (27), Reserved (28), Reserved (29), Reserved (30), Reserved (31), Reserved (32), Reserved (33), Reserved (34), Reserved (35), Reserved (36), Reserved (37), Reserved (38), Reserved (39), Reserved (40), Reserved (41), Reserved (42), Reserved (43), Reserved (44), Reserved (45), Reserved (46), Reserved (47), Reserved (48), Reserved (49), INT maths err (50), FLOAT maths err (51), Reserved (52), Reserved (53), Reserved (54), Reserved (55), Reserved (56), Reserved (57), Reserved (58), Reserved (59), Reserved (60), Reserved (61), Reserved (62), Reserved (63), Reserved (64), Reserved (65), Reserved (66), Reserved (67), Reserved (68), Reserved (69), Reserved (70), Reserved (71), Reserved (72), Reserved (73), Reserved (74), Reserved (75), Reserved (76), Reserved (77), Reserved (78), Reserved (79), Reserved (80), Reserved (81), Reserved (82), Reserved (83), Reserved (84), Reserved (85), Reserved (86), Reserved (87), Reserved (88), Reserved (89), Reserved (90), Reserved (91), Reserved (92), Reserved (93), Reserved (94), Reserved (95), Reserved (96), Reserved (97), Reserved (98), Reserved (99), Link Loss (100), E/IP Timeout (101), E/IP Read Param (102), E/IP Write Param (103), E/IP Fault (104), Modbus Timeout (105), Cyclic Timeout (106), Cyclic RX Late (107), INIT Switch (108), INIT PTP (109), INIT Cyclic (110), INIT Modbus (111), INIT SMTP (112), INIT Ethernet/IP (113), INIT TCP/IP (114), Ethernet Failure (115), E/IP PLC IDLE (116), Sync Task ORun (117), INIT Param Chann (118), Link Overload (119), MCast error (120), Reserved (121), Reserved (122), Reserved (123), Reserved (124), Reserved (125), Reserved (126), Reserved (127), Reserved (128), Reserved (129), Reserved (130), Reserved (131), Reserved (132), Reserved (133), Reserved (134), Reserved (135), Reserved (136), Reserved (137), Reserved (138), Reserved (139), Reserved (140), Reserved (141), Reserved (142), Reserved (143), Reserved (144), Reserved (145), Reserved (146), Reserved (147), Reserved (148), Reserved (149), Reserved (150), Reserved (151), Reserved (152), Reserved (153), Reserved (154), Reserved (155), Reserved (156), Reserved (157), Reserved (158), Reserved (159), Reserved (160), Reserved (161), Reserved (162), Reserved (163), Reserved (164), Reserved (165), Reserved (166), Reserved (167), Reserved (168), Reserved (169), Reserved (170), Reserved (171), Reserved (172), Reserved (173), Reserved (174), Reserved (175), Reserved (176), Reserved (177), Reserved (178), Reserved (179), Reserved (180), Reserved (181), Reserved (182), Reserved (183), Reserved (184), Reserved (185), Reserved (186), Reserved (187), Reserved (188), Reserved (189), Reserved (190), Reserved (191), Reserved (192), Reserved (193), Reserved (194), Reserved (195), Reserved (196), Reserved (197), Reserved (198), Reserved (199), SW Fault (200), BG Overrun (201), FW Invalid (202), Drv unknown (203), Drv unsupported (204), Mode unknown (205), Mode unsupported (206), FLASH Corrupt (207), Dbase Init (208), FS Init (209), Memory Alloc (210), Filesystem (211), Configuration (212), OHt (213), TO drv (214), eCMP (215), TO eCMP Slot1 (216), TO eCMP Slot2 (217), TO eCMP Slot3 (218), TO eCMP Slot4 (219), Output Overload (220), Factory Settings (221), Functional Test (222), Config Restore (223), Self Test Error (224), Runtime Config (225), Processor except (226), Task Starvation (227), Runtime except (228), COM Overrun (229), Reserved (230), Reserved (231), Reserved (232), Reserved (233), Reserved (234), Reserved (235), Reserved (236), Reserved (237), Reserved (238), Reserved (239), Reserved (240), Reserved (241), Reserved (242), Reserved (243), Reserved (244), Reserved (245), Reserved (246), Reserved (247), Reserved (248), Reserved (249), Reserved (250), Reserved (251), Reserved (252), Reserved (253), Reserved (254), Reserved (255) |  | RO | Txt | ND | NC | PT |
3.01.050 | Run Time Error Task Id | System Watchdog (0), User FWheel task (1), User Clock0 task (2), User Clock1 task (3), User Clock2 task (4), User Clock3 task (5), User Pos task (6), User Init task (7), User event1 task (8), User event2 task (9), User event3 task (10), User event4 task (11), User error task (12), Unknown task (13), No error (14) |  | RO | Txt | ND | NC | PT |
3.01.051 | Run Time Error Area | 0 to 65535 |  | RO | Num | ND | NC | PT |
3.01.052 | Run Time Error Offset | 0 to 4294967295 |  | RO | Num | ND | NC | PT |
3.01.053 | User Application ID | 0 to 4294967295 | 0 | RO | Num |  | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |