# Menu 5 Single Line Descriptions − Regen Status

Mode: Regeneration

Parameter | Range | Default | Type
--- | --- | --- | ---
05.001 | Output Frequency | ±200.0 Hz |  | RO | Num | ND | NC | PT | FI
05.002 | Output Voltage | VM_AC_VOLTAGE[MIN] to VM_AC_VOLTAGE[MAX] V |  | RO | Num | ND | NC | PT | FI
05.003 | Output Power | VM_POWER[MIN] to VM_POWER[MAX] kW |  | RO | Num | ND | NC | PT | FI
05.004 | High Resolution Frequency | ±200.00 Hz |  | RO | Num | ND | NC | PT | FI
05.005 | D.c. Bus Voltage | VM_DC_VOLTAGE[MIN] to VM_DC_VOLTAGE[MAX] V |  | RO | Num | ND | NC | PT | FI
05.007 | Rated Current | VM_RATED_CURRENT[MIN] to VM_RATED_CURRENT[MAX] A | Default Current Rating A | RW | Num |  |  |  | US
05.018 | Maximum Switching Frequency | 0 to VM_SWITCHING_FREQUENCY kHz | 3 (1) kHz | RW | Txt |  |  |  | US
05.025 | A.c. Filter Capacitance | 0.0000 to 0.5000 mF | 0.0000 mF | RW | Num |  |  |  | US
05.026 | No‑load Power Offset | VM_POWER[MIN] to VM_POWER[MAX] kW | 0.000 kW | RW | Num |  |  |  | US
05.035 | Auto‑switching Frequency Change | Enabled (0), Disabled (1), No Ripple Detect (2) | Enabled (0) | RW | Txt |  |  |  | US
05.036 | Auto‑switching Frequency Step Size | 1 to 2 | 2 | RW | Num |  |  |  | US
05.037 | Switching Frequency | 2 (0), 3 (1), 4 (2), 6 (3), 8 (4), 12 (5), 16 (6) kHz |  | RO | Txt | ND | NC | PT |
05.038 | Minimum Switching Frequency | 0 to VM_MIN_SWITCHING_FREQUENCY kHz | 3 (1) kHz | RW | Txt |  |  |  | US
05.039 | Maximum Inverter Temperature Ripple | 20 to 60 °C | 60 °C | RW | Num |  |  |  | US
05.050 | Phase Voltage Input Select | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
05.051 | Input Voltage 1 | ±100.00 % |  | RW | Num | ND | NC |  |
05.052 | Input Voltage 2 | ±100.00 % |  | RW | Num | ND | NC |  |
05.053 | Input Voltage 3 | ±100.00 % |  | RW | Num | ND | NC |  |
05.056 | Voltage Feedback Ratio | 1.0 to 1000.0 | 100.0 | RW | Num |  |  |  | US
05.057 | Voltage Feedback Phase Shift | -180 to 179 ° | 0 ° | RW | Num |  |  |  | US
05.063 | Phase Voltage Monitor | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
05.064 | Vuv or Vu | ±1500 V |  | RO | Num | ND | NC | PT |
05.065 | Vvw or Vv | ±1500 V |  | RO | Num | ND | NC | PT |
05.066 | Vwu or Vw | ±1500 V |  | RO | Num | ND | NC | PT |
05.067 | Vu r.m.s. | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.068 | Vv r.m.s. | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.069 | Vw r.m.s. | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.070 | Vuv r.m.s. | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.071 | Vvw r.m.s. | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.072 | Vwu r.m.s. | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.074 | Grid Frequency | ±200.00 Hz |  | RO | Num | ND | NC | PT | FI
05.076 | Input Voltage 1 Trim | 0.9000 to 1.1000 | 1.0000 | RW | Num |  |  |  | US
05.077 | Input Voltage 2 Trim | 0.9000 to 1.1000 | 1.0000 | RW | Num |  |  |  | US
05.078 | Input Voltage 3 Trim | 0.9000 to 1.1000 | 1.0000 | RW | Num |  |  |  | US
05.080 | Vpos | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT |
05.081 | Vneg | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT |
05.082 | Measured Grid Voltage | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.085 | Voltage Feedback Select | Converter Output (0), Measured Grid (1) | Converter Output (0) | RW | Txt |  |  |  | US
05.086 | Vd | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.087 | Vq | 0 to VM_AC_VOLTAGE V |  | RO | Num | ND | NC | PT | FI
05.091 | Input Current 1 | ±100.00 % |  | RO | Num | ND | NC |  |
05.092 | Input Current 2 | ±100.00 % |  | RO | Num | ND | NC |  |
05.094 | Current Feedback Ratio | 0.01 to 1000.00 | 10.00 | RW | Num |  |  |  | US
05.095 | Current Feedback Phase Shift | -180 to 179 ° | 0 ° | RW | Num |  |  |  | US
05.096 | Iu | VM_DRIVE_CURRENT_PEAK[MIN] to VM_DRIVE_CURRENT_PEAK[MAX] A |  | RO | Num | ND | NC | PT |
05.097 | Iv | VM_DRIVE_CURRENT_PEAK[MIN] to VM_DRIVE_CURRENT_PEAK[MAX] A |  | RO | Num | ND | NC | PT |
05.098 | Iw | VM_DRIVE_CURRENT_PEAK[MIN] to VM_DRIVE_CURRENT_PEAK[MAX] A |  | RO | Num | ND | NC | PT |
05.099 | Iu r.m.s. | VM_DRIVE_CURRENT[MIN] to VM_DRIVE_CURRENT[MAX] A |  | RO | Num | ND | NC | PT | FI
05.100 | Iv r.m.s. | VM_DRIVE_CURRENT[MIN] to VM_DRIVE_CURRENT[MAX] A |  | RO | Num | ND | NC | PT | FI
05.101 | Iw r.m.s. | VM_DRIVE_CURRENT[MIN] to VM_DRIVE_CURRENT[MAX] A |  | RO | Num | ND | NC | PT | FI
05.103 | Current Feedback Select | Converter Output (0), Measured Grid (1) | Converter Output (0) | RW | Txt |  |  |  | US
05.104 | Id | VM_DRIVE_CURRENT[MIN] to VM_DRIVE_CURRENT[MAX] A |  | RO | Num | ND | NC | PT | FI
05.105 | Iq | VM_DRIVE_CURRENT[MIN] to VM_DRIVE_CURRENT[MAX] A |  | RO | Num | ND | NC | PT | FI

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |