# Slot 3 Menu 10 Single Line Descriptions − RTMOE Easy Mode

Mode: RFC‑S

Parameter | Range | Default | Type
--- | --- | --- | ---
3.10.001 | Easy Mode Enable | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US
3.10.002 | Easy Mode Reset | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
3.10.003 | Easy Mode Default | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
3.10.004 | Cyclic Messages Per Second | 0 to 65535 |  | RO | Num | ND | NC | PT |
3.10.005 | Configuration Valid | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
3.10.006 | Operational | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
3.10.007 | Active Configuration | None (0), Easy Mode (1), Advanced (2) |  | RO | Txt | ND | NC | PT |
3.10.008 | Timeout Count | 0 to 65535 |  | RO | Num | ND | NC | PT |
3.10.009 | Data Late Count | 0 to 65535 |  | RO | Num | ND | NC | PT |
3.10.010 | Tx1 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
3.10.011 | Tx1 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
3.10.012 | Tx1 Source Parameter | 0 to 499999 | 0 | RW | Num |  |  | PT | US
3.10.013 | Tx1 Parameter Count | 0 to 20 | 0 | RW | Num |  |  |  | US
3.10.014 | Tx1 Link Transmission Type | Unicast (0), Broadcast (1), Multicast1 (2), Multicast2 (3), Multicast3 (4), Multicast4 (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Unicast (0) | RW | Txt |  |  |  | US
3.10.015 | Tx1 Destination Address | 0.0.0.0 to 255.255.255.255 | 0.0.0.0 | RW | IP |  |  |  | US
3.10.016 | Tx1 Message Period | 0 to 100 ms | 0 ms | RW | Num |  |  |  | US
3.10.019 | Tx1 Link Status | Multicast limit (-32), Disabled (-31), VLAN disabled (-30), Reserved 29 (-29), Reserved 28 (-28), Reserved 27 (-27), Reserved 26 (-26), Reserved 25 (-25), Reserved 24 (-24), Reserved 23 (-23), Invalid DST IP (-22), SYNC unsupported (-21), MEC offset (-20), Invalid tx rate (-19), Too many mapping (-18), Link busy (-17), Invalid profile (-16), Invalid mapping (-15), Read only param (-14), Msg mismatch (-13), Msg too long (-12), Attrib NA (-11), Attrib RO (-10), Attrib missing (-9), Timeout (-8), In error (-7), Link num in use (-6), Not editable (-5), Invalid link num (-4), Invalid args (-3), Too many links (-2), Out of memory (-1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
3.10.020 | Tx2 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
3.10.021 | Tx2 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
3.10.022 | Tx2 Source Parameter | 0 to 499999 | 0 | RW | Num |  |  | PT | US
3.10.023 | Tx2 Parameter Count | 0 to 20 | 0 | RW | Num |  |  |  | US
3.10.024 | Tx2 Link Transmission Type | Unicast (0), Broadcast (1), Multicast1 (2), Multicast2 (3), Multicast3 (4), Multicast4 (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Unicast (0) | RW | Txt |  |  |  | US
3.10.025 | Tx2 Destination Address | 0.0.0.0 to 255.255.255.255 | 0.0.0.0 | RW | IP |  |  |  | US
3.10.026 | Tx2 Message Period | 0 to 100 ms | 0 ms | RW | Num |  |  |  | US
3.10.029 | Tx2 Link Status | Multicast limit (-32), Disabled (-31), VLAN disabled (-30), Reserved 29 (-29), Reserved 28 (-28), Reserved 27 (-27), Reserved 26 (-26), Reserved 25 (-25), Reserved 24 (-24), Reserved 23 (-23), Invalid DST IP (-22), SYNC unsupported (-21), MEC offset (-20), Invalid tx rate (-19), Too many mapping (-18), Link busy (-17), Invalid profile (-16), Invalid mapping (-15), Read only param (-14), Msg mismatch (-13), Msg too long (-12), Attrib NA (-11), Attrib RO (-10), Attrib missing (-9), Timeout (-8), In error (-7), Link num in use (-6), Not editable (-5), Invalid link num (-4), Invalid args (-3), Too many links (-2), Out of memory (-1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
3.10.030 | Tx3 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
3.10.031 | Tx3 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
3.10.032 | Tx3 Source Parameter | 0 to 499999 | 0 | RW | Num |  |  | PT | US
3.10.033 | Tx3 Parameter Count | 0 to 20 | 0 | RW | Num |  |  |  | US
3.10.034 | Tx3 Link Transmission Type | Unicast (0), Broadcast (1), Multicast1 (2), Multicast2 (3), Multicast3 (4), Multicast4 (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Unicast (0) | RW | Txt |  |  |  | US
3.10.035 | Tx3 Destination Address | 0.0.0.0 to 255.255.255.255 | 0.0.0.0 | RW | IP |  |  |  | US
3.10.036 | Tx3 Message Period | 0 to 100 ms | 0 ms | RW | Num |  |  |  | US
3.10.039 | Tx3 Link Status | Multicast limit (-32), Disabled (-31), VLAN disabled (-30), Reserved 29 (-29), Reserved 28 (-28), Reserved 27 (-27), Reserved 26 (-26), Reserved 25 (-25), Reserved 24 (-24), Reserved 23 (-23), Invalid DST IP (-22), SYNC unsupported (-21), MEC offset (-20), Invalid tx rate (-19), Too many mapping (-18), Link busy (-17), Invalid profile (-16), Invalid mapping (-15), Read only param (-14), Msg mismatch (-13), Msg too long (-12), Attrib NA (-11), Attrib RO (-10), Attrib missing (-9), Timeout (-8), In error (-7), Link num in use (-6), Not editable (-5), Invalid link num (-4), Invalid args (-3), Too many links (-2), Out of memory (-1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
3.10.040 | Rx1 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
3.10.041 | Rx1 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
3.10.042 | Rx1 Destination Parameter | 0 to 499999 | 0 | RW | Num |  |  |  | US
3.10.043 | Rx1 Parameter Count | 0 to 20 | 0 | RW | Num |  |  |  | US
3.10.044 | Rx1 Source Type | Direct (0), Multicast1 (1), Multicast2 (2), Multicast3 (3), Multicast4 (4), Local (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Direct (0) | RW | Txt |  |  |  | US
3.10.045 | Rx1 Timeout | 0 to 65535 ms | 100 ms | RW | Num |  |  |  | US
3.10.046 | Rx1 Timeout Action | Trip (0), Clear output (1), Hold last (2) | Trip (0) | RW | Txt |  |  |  | US
3.10.048 | Rx1 Timeout Event Type | No Event (0), Event 0 (1), Event 1 (2), Event 2 (3), Event 3 (4) | No Event (0) | RW | Txt |  |  |  | US
3.10.049 | Rx1 Link Status | Multicast limit (-32), Disabled (-31), VLAN disabled (-30), Reserved 29 (-29), Reserved 28 (-28), Reserved 27 (-27), Reserved 26 (-26), Reserved 25 (-25), Reserved 24 (-24), Reserved 23 (-23), Invalid DST IP (-22), SYNC unsupported (-21), MEC offset (-20), Invalid tx rate (-19), Too many mapping (-18), Link busy (-17), Invalid profile (-16), Invalid mapping (-15), Read only param (-14), Msg mismatch (-13), Msg too long (-12), Attrib NA (-11), Attrib RO (-10), Attrib missing (-9), Timeout (-8), In error (-7), Link num in use (-6), Not editable (-5), Invalid link num (-4), Invalid args (-3), Too many links (-2), Out of memory (-1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
3.10.050 | Rx2 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
3.10.051 | Rx2 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
3.10.052 | Rx2 Destination Parameter | 0 to 499999 | 0 | RW | Num |  |  |  | US
3.10.053 | Rx2 Parameter Count | 0 to 20 | 0 | RW | Num |  |  |  | US
3.10.054 | Rx2 Source Type | Direct (0), Multicast1 (1), Multicast2 (2), Multicast3 (3), Multicast4 (4), Local (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Direct (0) | RW | Txt |  |  |  | US
3.10.055 | Rx2 Timeout | 0 to 65535 ms | 100 ms | RW | Num |  |  |  | US
3.10.056 | Rx2 Timeout Action | Trip (0), Clear output (1), Hold last (2) | Trip (0) | RW | Txt |  |  |  | US
3.10.058 | Rx2 Timeout Event Type | No Event (0), Event 0 (1), Event 1 (2), Event 2 (3), Event 3 (4) | No Event (0) | RW | Txt |  |  |  | US
3.10.059 | Rx2 Link Status | Multicast limit (-32), Disabled (-31), VLAN disabled (-30), Reserved 29 (-29), Reserved 28 (-28), Reserved 27 (-27), Reserved 26 (-26), Reserved 25 (-25), Reserved 24 (-24), Reserved 23 (-23), Invalid DST IP (-22), SYNC unsupported (-21), MEC offset (-20), Invalid tx rate (-19), Too many mapping (-18), Link busy (-17), Invalid profile (-16), Invalid mapping (-15), Read only param (-14), Msg mismatch (-13), Msg too long (-12), Attrib NA (-11), Attrib RO (-10), Attrib missing (-9), Timeout (-8), In error (-7), Link num in use (-6), Not editable (-5), Invalid link num (-4), Invalid args (-3), Too many links (-2), Out of memory (-1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
3.10.060 | Rx3 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
3.10.061 | Rx3 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
3.10.062 | Rx3 Destination Parameter | 0 to 499999 | 0 | RW | Num |  |  |  | US
3.10.063 | Rx3 Parameter Count | 0 to 20 | 0 | RW | Num |  |  |  | US
3.10.064 | Rx3 Source Type | Direct (0), Multicast1 (1), Multicast2 (2), Multicast3 (3), Multicast4 (4), Local (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Direct (0) | RW | Txt |  |  |  | US
3.10.065 | Rx3 Timeout | 0 to 65535 ms | 100 ms | RW | Num |  |  |  | US
3.10.066 | Rx3 Timeout Action | Trip (0), Clear output (1), Hold last (2) | Trip (0) | RW | Txt |  |  |  | US
3.10.068 | Rx3 Timeout Event Type | No Event (0), Event 0 (1), Event 1 (2), Event 2 (3), Event 3 (4) | No Event (0) | RW | Txt |  |  |  | US
3.10.069 | Rx3 Link Status | Multicast limit (-32), Disabled (-31), VLAN disabled (-30), Reserved 29 (-29), Reserved 28 (-28), Reserved 27 (-27), Reserved 26 (-26), Reserved 25 (-25), Reserved 24 (-24), Reserved 23 (-23), Invalid DST IP (-22), SYNC unsupported (-21), MEC offset (-20), Invalid tx rate (-19), Too many mapping (-18), Link busy (-17), Invalid profile (-16), Invalid mapping (-15), Read only param (-14), Msg mismatch (-13), Msg too long (-12), Attrib NA (-11), Attrib RO (-10), Attrib missing (-9), Timeout (-8), In error (-7), Link num in use (-6), Not editable (-5), Invalid link num (-4), Invalid args (-3), Too many links (-2), Out of memory (-1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |