# Menu 1 Single Line Descriptions − Grid Control

Mode: Regeneration

Parameter | Range | Default | Type
--- | --- | --- | ---
01.001 | Grid Power (P) | VM_POWER[MIN] to VM_POWER[MAX] kW |  | RO | Num | ND | NC | PT | FI
01.002 | Grid VARs (Q) | VM_POWER[MIN] to VM_POWER[MAX] kVAr |  | RO | Num | ND | NC | PT | FI
01.003 | Regen Sub‑mode | AFE (0), Generator (1) | AFE (0) | RW | Txt |  |  |  | US
01.004 | Grid Power/VARs Filter Disable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
01.010 | Grid Mode | Grid Connected (0), Grid Forming (1), Grid Supporting (2) | Grid Connected (0) | RW | Txt |  |  |  | US
01.011 | Action On Phase Loss | No Action (0), Fault Detect (1), Trip (2) | Trip (2) | RW | Txt |  |  |  | US
01.012 | Action On Phase Imbalance | No Action (0), Fault Detect (1), Trip (2) | Trip (2) | RW | Txt |  |  |  | US
01.013 | Action On Island Detected | No Action (0), Fault Detect (1), Trip (2) | Trip (2) | RW | Txt |  |  |  | US
01.014 | Faults Active | 0000 to 1111 |  | RO | Bin | ND | NC | PT |
01.015 | Action On Fault | Trip (0), Grid Forming (1), Grid Supporting (2) | Trip (0) | RW | Txt |  |  |  | US
01.016 | Action on Fault Recovery | Disabled (0), Recover (1) | Disabled (0) | RW | Txt |  |  |  | US
01.017 | Fault Ride‑through Time | 0.0 to 5.0 s | 0.0 s | RW | Num |  |  |  | US
01.018 | Connect grid | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
01.019 | Grid Contactor Operating Time | 0 to 500 ms | 100 ms | RW | Num |  |  |  | US
01.020 | Grid‑mode Changeover State | Connected (0), From Connected (1), Forming (2), Supporting (3), To Connected (4) |  | RO | Txt | ND | NC | PT |
01.030 | A.c Voltage Set‑point | 0 to VM_AC_VOLTAGE_SET V | 200V drive: 200 V 400V drive 50Hz: 400 V 400V drive 60Hz: 460 V | RW | Num |  | RA |  | US
01.031 | Transformer Inductance | 0.000 to 50.000 mH | 0.000 mH | RW | Num |  |  |  | US
01.033 | A.c. Voltage Controller Gain | 0 to 1000 | 100 | RW | Num |  |  |  | US
01.034 | Voltage Droop | 0.00 to 50.00 % | 5.00 % | RW | Num |  |  |  | US
01.035 | Voltage Offset | ±1000 V |  | RO | Num | ND | NC |  |
01.036 | Voltage Offset Reset Rate | 0.00 to 100.00 s/100V | 1.00 s/100V | RW | Num |  |  |  | US
01.037 | Voltage Set‑point Ramp Rate | 0.00 to 100.00 s/100V |  | RW | Num | ND |  |  |
01.038 | Converter Output As Feedback | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US
01.040 | Frequency Set‑point | ±200.00 Hz | 50Hz: 50.00 Hz 60Hz: 60.00 Hz | RW | Num |  |  |  | US
01.041 | Frequency Droop | 0.00 to 50.00 % | 5.00 % | RW | Num |  |  |  | US
01.042 | Frequency Offset | ±400.00 Hz |  | RO | Num | ND | NC |  |
01.043 | Frequency Offset Reset Rate | 0.00 to 100.00 s/100Hz | 1.00 s/100Hz | RW | Num |  |  |  | US
01.044 | Frequency Set‑point Ramp Rate | 0.00 to 100.00 s/100Hz | 1.00 s/100Hz | RW | Num |  |  |  | US
01.050 | Start Mode | Active Start (0), Black Start Once (1), Black Start (2) | Active Start (0) | RW | Txt |  |  |  | US
01.051 | Black Start Voltage Ramp Rate | 0.00 to 100.00 s/100V | 1.00 s/100V | RW | Num |  |  |  | US
01.052 | Black‑start active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |