# Slot 3 Menu 0 − MCi Setup

Mode: Open‑Loop

Parameter | 3.00.001 Module ID
--- | ---
Short description | Module ID
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

The Module ID. Next Generation Apps = nnn.

Parameter | 3.00.002 Software Version
--- | ---
Short description | Software Version
Minimum | 0 | Maximum | 99999999
Default |  | Units |
Type | 32 Bit Volatile | Update Rate |
Display Format | Version | Decimal Places | 0
Coding | RO, ND, NC, PT

Module firmware version in ww.xx.yy.zz format

Parameter | 3.00.003 Hardware Version
--- | ---
Short description | Hardware Version
Minimum | 0.00 | Maximum | 99.99
Default |  | Units |
Type | 16 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 2
Coding | RO, ND, NC, PT

Parameter | 3.00.004 Serial Number LS
--- | ---
Short description |
Minimum | 0 (Display: 00000000) | Maximum | 99999999 (Display: 99999999)
Default |  | Units |
Type | 32 Bit Volatile | Update Rate |
Display Format | Lead Zero Pad | Decimal Places | 0
Coding | RO, ND, NC, PT

Least significant 8 digits of the module's serial number.

Parameter | 3.00.005 Serial Number MS
--- | ---
Short description |
Minimum | 0 | Maximum | 99999999
Default |  | Units |
Type | 32 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Parameter | 3.00.006 Module Status
--- | ---
Short description |
Minimum | -2 | Maximum | 3
Default |  | Units |
Type | 8 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 0
Coding | RO, TE, ND, NC, PT

Value | Text | Description
-2 | Bootldr - Update | The bootloader is performing a flash update.
-1 | Bootldr - Idle | The bootloader is idle.
0 | Initialising |
1 | OK | Module is initialised with no errors present
2 | Config | A configuration error has been detected
3 | Error | An error has occured preventing the module from running correctly

Parameter | 3.00.007 Reset Module
--- | ---
Short description |
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 0
Coding | RW, NC

Parameter | 3.00.008 Default Module
--- | ---
Short description |
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 0
Coding | RW, NC

Parameter | 3.00.009 Active Alarm Bits
--- | ---
Short description |
Minimum | 0 (Display: 0000000000000000) | Maximum | 65535 (Display: 1111111111111111)
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | Background
Display Format | Binary | Decimal Places | 0
Coding | RO, ND, NC, BU

Parameter | 3.00.010 Active IP Address
--- | ---
Short description |
Minimum | -2147483648 (Display: 128.0.0.0) | Maximum | 2147483647 (Display: 127.255.255.255)
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | Background
Display Format | IP Address | Decimal Places | 0
Coding | RO, ND, NC, PT

Modules active IP address.

Parameter | 3.00.030 Slot Indicator
--- | ---
Short description |
Minimum | 0 | Maximum | 8
Default |  | Units |
Type | 8 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

Provides the slot number (logical slot 1, 2, or 3) into which this option module is installed.

Parameter | 3.00.031 Slot Menu Number
--- | ---
Short description |
Minimum | 0 | Maximum | 255
Default |  | Units |
Type | 8 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

Provides the menu number for the basic setup menu for this option module.

Parameter | 3.00.036 Inhibit User Program Start
--- | ---
Short description |
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Read at module startup
Display Format | Standard | Decimal Places | 0
Coding | RW, NC, PT

This parameter can be used to recover the module from a recurrent (user application) catastrophic failure.

If the user application causes the MCi2x0 module to encounter a non-resettable exception then the option module parameters (Slot.mm.ppp) become unavailable via the keypad or communications interface. This parameter resides in the drive's database in menu 15/16/17 and can be used to force the user program to NOT be started regardless of the Autorun parameter the next time the module is started.

Procedure:

1) Set 15/16/17.036.

2) Save drive parameters (e.g. by setting 00.000 to 1000 or 1001 if the drive is in under-voltage state, and pressing the reset button. The precise sequence may vary from drive to drive.)

3) Cause a cold start of the MCi2x0 module. The simplest way to achieve this is to power down the drive.

4) When the MCi210 firmware starts running it checks this parameter and uses it as a master override to decline to start the user application. If the parameter is set the module clears it and saves the drive parameters.

Please be aware that this sequence saves drive parameters and therefore may modify any parameter whose present value does not match its saved value.

Parameter | 3.00.037 Program Status
--- | ---
Short description | This parameter displays the status of the user program
Minimum | 0 | Maximum | 3
Default |  | Units |
Type | 8 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, TE, ND, NC, PT, BU

This parameter indicates the status of a user program, if it is present. If no user program is present in the module then it will also indicate this.

If the status indicates a runtime error (3, Error) the user's Error task may be running otherwise the user program will have stopped.

Value | Text | Description
0 | None | No user program is present
1 | Stopped | The user program is not running
2 | Run | The user program is running
3 | Error | Runtime error.

If the module contains a user program this parameter displays its status otherwise it displays 0 (no program present).