# Menu 10 Single Line Descriptions − Status and Trips

Mode: Regeneration

Parameter | Range | Default | Type
--- | --- | --- | ---
10.001 | Drive Healthy | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.002 | Drive Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.008 | Rated Load Reached | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.009 | Current Limit Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.010 | Regenerating | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.011 | Braking IGBT Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.012 | Braking Resistor Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.015 | Supply Loss | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.016 | Under Voltage Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.017 | Inductor Overload Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.018 | Drive Over‑temperature Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.019 | Drive Warning | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.020 | Trip 0 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.021 | Trip 1 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.022 | Trip 2 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.023 | Trip 3 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.024 | Trip 4 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.025 | Trip 5 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.026 | Trip 6 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.027 | Trip 7 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.028 | Trip 8 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.029 | Trip 9 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.030 | Braking Resistor Rated Power | 0.000 to 99999.999 kW | Default Brake Resistor Rated Power kW | RW | Num |  |  |  | US
10.031 | Braking Resistor Thermal Time Constant | 0.000 to 1500.000 s | Default Brake Thermal TC s | RW | Num |  |  |  | US
10.032 | External Trip | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
10.033 | Drive Reset | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
10.034 | Number Of Auto‑reset Attempts | None (0), 1 (1), 2 (2), 3 (3), 4 (4), 5 (5), Infinite (6) | None (0) | RW | Txt |  |  |  | US
10.035 | Auto‑reset Delay | 1.0 to 600.0 s | 1.0 s | RW | Num |  |  |  | US
10.036 | Auto‑reset Hold Drive Healthy | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
10.037 | Action On Trip Detection | 00000 to 11111 | 00000 | RW | Bin |  |  |  | US
10.038 | User Trip | 0 to 255 |  | RW | Num | ND | NC |  |
10.039 | Braking Resistor Thermal Accumulator | 0.0 to 100.0 % |  | RO | Num | ND | NC | PT |
10.040 | Status Word | 0 to 32767 |  | RO | Num | ND | NC | PT |
10.041 | Trip 0 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.042 | Trip 0 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.043 | Trip 1 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.044 | Trip 1 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.045 | Trip 2 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.046 | Trip 2 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.047 | Trip 3 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.048 | Trip 3 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.049 | Trip 4 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.050 | Trip 4 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.051 | Trip 5 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.052 | Trip 5 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.053 | Trip 6 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.054 | Trip 6 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.055 | Trip 7 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.056 | Trip 7 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.057 | Trip 8 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.058 | Trip 8 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.059 | Trip 9 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.060 | Trip 9 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.061 | Braking Resistor Resistance | 0.00 to 10000.00 Ω | Default Brake Resistor Ω | RW | Num |  |  |  | US
10.063 | Local Keypad Battery Low | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.064 | Remote Keypad Battery Low | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.065 | Auto‑tune Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.067 | Fire Mode Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.068 | Hold Drive Healthy on Under Voltage | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
10.069 | Additional Status Bits | 0 to 1023 |  | RO | Num | ND | NC | PT |
10.070 | Trip 0 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.071 | Trip 1 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.072 | Trip 2 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.073 | Trip 3 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.074 | Trip 4 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.075 | Trip 5 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.076 | Trip 6 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.077 | Trip 7 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.078 | Trip 8 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.079 | Trip 9 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.081 | Phase Loss | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.082 | Phase Imbalance | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.083 | Island Detected | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.084 | Reactive Current Limit Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.089 | Additional Status Bits 2 | 00000000 to 11111111 |  | RO | Bin | ND | NC | PT |
10.101 | Drive Status | Inhibit (0), Ready (1), Stop (2), Synchronising (3), Run (4), Supply Loss (5), Deceleration (6), dc Injection (7), Position (8), Trip (9), Active (10), Off (11), Hand (12), Auto (13), Heat (14), Under Voltage (15), Phasing (16), Black Start (17) |  | RO | Txt | ND | NC | PT |
10.102 | Trip Reset Source | 0 to 1023 |  | RO | Num | ND | NC | PT | PS
10.103 | Trip Time Identifier | -2147483648 to 2147483647 ms |  | RO | Num | ND | NC | PT |
10.104 | Active Alarm | None (0), Brake Resistor (1), Motor Overload (2), Ind Overload (3), Drive Overload (4), Auto Tune (5), Limit Switch (6), Fire Mode (7), Low Load (8), Option Slot 1 (9), Option Slot 2 (10), Option Slot 3 (11), Option Slot 4 (12) |  | RO | Txt | ND | NC | PT |
10.106 | Potential Drive Damage Conditions | 0000 to 1111 |  | RO | Bin | ND | NC | PT | PS
10.107 | Auto‑tune State | Not Active (0), Resistance (1), pLs (2), Ls (3), Flux (4), Flux Repeat (5), Ld Lq No‑load (6), Lq (7), Ke (8), Inertia (9) |  | RO | Txt | ND | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |